THERMOSTAT ADJUSTMENT
1. Unplug the popcorn machine from the AC outlet. 

2. Remove the kettle from the machine by: 

a. Putting kettle in the “OPEN” position (hanging) 

b. Unplug the kettle pigtail from the ceiling of the popper 

c. Pull the clip from the hinge pin and remove the pin 

d. The kettle will now be free 

3. Place the kettle upside-down on a flat surface. 

4. Remove the two acorn nuts using a 3/8” wrench and the two elbow screws using a screwdriver (see figure 1). 

5. You will now be able to slide the outer jacket away from the kettle inner (see figure 2) 

6. Adjust the thermostat temperature screw with a straight blade screwdriver (see figure 3)

by: 

a. Notice the color of the insulator rings in the thermostat. The rings will be either pink or white. Locate adjustment screw in thermostat. (figure 3) 

b. To increase heat for pink insulator turn counter clockwise, for white insulator turn clockwise. (¼ turn will change temperature approximately 40 degrees)

c. To decrease heat for pink insulator turn clockwise, for white insulator turn counter clockwise. (¼ turn will change temperature approximately 40 degrees)
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     FIGURE 1




FIGURE 2 
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FIGURE 3 
Re-assemble the kettle by reversing the instructions.
